+------------------------------------+
| FTV100 FIRMWARE V2.1.6 (2012-03-20) |
|	GREENREPORT V4.5	      |
+-------------------------------------+

This ZIP archive contains the following files :

- Upgrade Procedure FTV100 V1 EN.pdf
- Setup_UpLoaderGreenTest_v21.exe
- Setup_UpLoaderGreenTest_v30.exe
- FTV100_PREPARAZIONE_VARIANTE_1.hex
- FV_216.hex
- Setup_GREENREPORT_V4-5.exe
- CDM 2.04.16 WHQL Certified.zip
- How to install USB serial driver.pdf
- Read-Me First.txt


1) All those files must be extracted in the same directory
2) Run "Setup_UpLoaderGreenTestL_v21uo.exe"
3) Follow the instructions...



Note: this firmware version is compatible with a V4.5 GreenReport software version.




+------------------+
| Revision history |
+------------------+

Firmware 2.1.6
-------------
- (Bug fix) Temperature value display conditions fixed 


Firmware 2.1.5
-------------
- (New) Add the PRp parameter according EN61724 standard
- (New) Add the UPS power parameter in the instalation menu
- (New) Support the remote module version 2.0.0 (with a serial number sticker)


Firmware 2.1.4
-------------
- (Modification) Increase the measures stability
- (Modification) Increase the efficiency calculation
- (Modification) Increase the Prolongé par une seconde l’écran pendant l’allumage
- (Modification) Changement mots concernant la langue allemand
- (Modification) Add in the Setup menu the BOOT LOADER version


Firmware 2.1.3
-------------
- (Bug fix) Wrong data measures transfer


Firmware 2.1.2
-------------- 
- (Modification) Suppress the temperature coefficient limitation at 0,85
- (Modification) Suppress the display delay


Firmware 2.1.1
-------------- 
- (Modification) Add a temperature coefficient limitation at 0,85


Firmware 2.1.0
-------------- 
- (bug fix) Bad test pass in DC 
- (bug fix) When some AC or DC inputs are non actives, communication error
- (Modification) Add a display delay
- (Modification) Suppress the temperature coefficient limitation at 0,85
- (Modification) Increase the waiting time delay for the remote module communication before disconnection


Firmware 2.06
-------------
- (New features) Compatible with GreenReport V3.1.
- (bug fix) Random reset


Firmware 2.05
------------
- (bug fix) Bugs fixed.
- (Modification) Multilaguage texts


Firmware 2.02
------------

Initial release.
